{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["表1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"表1","index":0,"n_rows":35,"n_cols":12,"rows_kept":35,"merged":[[0,0,0,8],[0,9,0,11],[1,0,3,0],[1,1,3,2],[1,3,3,4],[1,5,3,5],[1,6,3,7],[1,8,1,11],[2,8,3,9],[2,10,3,10],[2,11,3,11],[4,1,4,2],[4,3,4,4],[4,6,4,7],[4,8,4,9],[5,1,5,2],[5,3,5,4],[5,6,5,7],[5,8,5,9],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[9,1,9,2],[9,3,9,4],[9,6,9,7],[9,8,9,9],[10,1,10,2],[10,3,10,4],[10,6,10,7],[10,8,10,9],[11,1,11,2],[11,3,11,4],[11,6,11,7],[11,8,11,9],[12,1,12,2],[12,3,12,4],[12,6,12,7],[12,8,12,9],[13,1,13,2],[13,3,13,4],[13,6,13,7],[13,8,13,9],[14,1,14,2],[14,3,14,4],[14,6,14,7],[14,8,14,9],[15,1,15,2],[15,3,15,4],[15,6,15,7],[15,8,15,9],[16,1,16,2],[16,3,16,4],[16,6,16,7],[16,8,16,9],[17,1,17,2],[17,3,17,4],[17,6,17,7],[17,8,17,9],[18,1,18,2],[18,3,18,4],[18,6,18,7],[18,8,18,9],[19,1,19,2],[19,3,19,4],[19,6,19,7],[19,8,19,9],[20,1,20,2],[20,3,20,4],[20,6,20,7],[20,8,20,9],[21,1,21,2],[21,3,21,4],[21,6,21,7],[21,8,21,9],[22,1,22,2],[22,3,22,4],[22,6,22,7],[22,8,22,9],[23,1,23,2],[23,3,23,4],[23,6,23,7],[23,8,23,9],[24,1,24,2],[24,3,24,4],[24,6,24,7],[24,8,24,9],[25,1,25,2],[25,3,25,4],[25,6,25,7],[25,8,25,9],[26,1,26,2],[26,3,26,4],[26,6,26,7],[26,8,26,9],[27,1,27,2],[27,3,27,4],[27,6,27,7],[27,8,27,9],[28,1,28,2],[28,3,28,4],[28,6,28,7],[28,8,28,9],[29,1,29,2],[29,3,29,4],[29,6,29,7],[29,8,29,9],[30,1,30,2],[30,3,30,4],[30,6,30,7],[30,8,30,9],[31,1,31,2],[31,3,31,4],[31,6,31,7],[31,8,31,9],[32,1,32,2],[32,3,32,4],[32,6,32,7],[32,8,32,9],[33,1,33,2],[33,3,33,4],[33,6,33,7],[33,8,33,9],[34,1,34,2],[34,3,34,4],[34,6,34,7],[34,8,34,9]],"flags":["formulas_cached_only"]}
["附件一"]
["序号","项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","备注"]
[]
[null,"强电系统"]
[1,"电能表集中采集系统安装调试 单相电度表安装",null,"1.名称：电度表\n2.规格型号：5（60）A\n3.含电度表接线\n4.备注：满足招标文件、图纸设计及施工规范要求",null,"块",1]
[2,"电能表集中采集系统安装调试 单相电度表调试",null,"1.名称：电度表调试\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"块",1]
[3,"DZ自动空气断路器安装 额定电流≤30A",null,"1.名称：断路器\n2.规格型号：MCB 63 1P-C16\n3.含断路器接线\n4.备注：满足招标文件、图纸设计及施工规范要求",null,"个",1]
[4,"DZ自动空气断路器安装 额定电流≤30A",null,"1.名称：断路器\n2.规格型号：RCB 2P-C20/0.03\n3.含断路器接线\n4.备注：满足招标文件、图纸设计及施工规范要求",null,"个",8]
[5,"套接紧定式镀锌钢导管(JDG)敷设 砖、混凝土结构明配 外径20mm",null,"1.名称：配管（明敷）\n2.规格型号：JDG20，含管卡\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",1.956]
[6,"塑料管敷设 刚性阻燃管敷设 砖、混凝土结构暗配 外径25mm",null,"1.名称：配管（暗敷）\n2.规格型号：PC25\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",8.253]
[7,"塑料管敷设 刚性阻燃管敷设 砖、混凝土结构暗配 外径20mm",null,"1.名称：配管（暗敷）\n2.规格型号：PC20\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",0.5]
[8,"管内穿线 穿照明线 铜芯 导线截面≤4mm2",null,"1.名称：管内穿线\n2.规格型号：WDZ-BYJ-4mm2\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",25.959]
[9,"管内穿线 穿照明线 铜芯 导线截面≤2.5mm2",null,"1.名称：管内穿线\n2.规格型号：WDZ-BYJ-2.5mm2\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",7.668]
[10,"荧光灯具安装 吸顶式 单管",null,"1.名称：铝制LED线性灯\n2.规格：20w\n3.备注：满足招标文件、\n图纸设计及施工规范要求",null,"套",15]
[11,"普通插座安装 单相 暗插座电流≤15A",null,"1.名称：五孔插座（暗装）\n2.规格：16A\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"套",15]
[12,"明装普通接线盒",null,"1.名称：接线盒（铁质）\n2.规格：86系列\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",15]
[13,"暗装开关(插座)盒",null,"1.名称：插座盒（塑料）\n2.规格：86系列\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",19]
[14,"剔槽及恢复",null,"1.名称：剔槽及恢复\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",5]
[15,"无端子外部接线≤6mm2",null,"1.名称：无端子外部接线≤6mm2\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"个",24]
[16,"无端子外部接线≤2.5mm2",null,"1.名称：无端子外部接线≤2.5mm2\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"个",3]
[null,"弱电系统"]
[1,"塑料管敷设 刚性阻燃管敷设 砖、混凝土结构暗配 外径20mm",null,"1.名称：配管（暗敷）\n2.规格型号：PC20\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",15]
[2,"双绞线缆 管内穿放 ≤4对",null,"1.名称：双绞线\n2.规格型号：UTP-CAT6E-4P\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",15]
[3,"光纤信息插座 单口",null,"1.名称：网络插座\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"个",1]
[4,"暗装开关(插座)盒",null,"1.名称：插座盒（塑料）\n2.规格：86系列\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",1]
[null,"设备采购"]
[1,"收银设备",null,"1.名称：收银设备\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"台",1]
[2,"超高频主机",null,"1.名称：超高频主机\n2.适用范围：图书馆、资料室、商超服装等应用场景\n3.规格：18.9*9.2*2.5CM，重量：348g，报警精准：全数字读取，一主机最多支持4个感应天线\n4.备注：满足招标文件、图纸设计及施工规范要求",null,"台",4]
[3,"极化天线",null,"1.名称：极化天线\n2.规格：频率范围：902MHz-928MHz极化方式，圆极化增益（dBi），>9DBi颜色：乳白色\n3.安装方式：抱杆（最大抱杆直径50mm）\n4.尺寸：25.8*25.8*4.3CM\n5.备注：满足招标文件、图纸设计及施工规范要求",null,"套",4]
[4,"充消磁器",null,"1.名称：充消磁器\n2.规格：读写方式：智能读写工作频率：860-868MHz/902-928MHz，支持USB接口\n3.尺寸：13.9*2.5CM\n4.备注：满足招标文件、图纸设计及施工规范要求",null,"台",1]
[5,"感应磁条",null,"1.名称：感应磁条\n2.规格：芯片类型：MR6-P工作频率：860MHz-960MHz，材质工艺：湿inlay-(双面背胶)\n3.尺寸：65*35mm\n4.备注：满足招标文件、图纸设计及施工规范要求",null,"个",5000]
[null,"安装费用"]
[1,"电气设备安装工程 措施项目 脚手架搭拆费",{"$nulls":3},"项",1]
[2,"建筑智能化工程 脚手架搭拆费",{"$nulls":3},"项",1]