{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["表3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"表3","index":0,"n_rows":27,"n_cols":12,"rows_kept":27,"merged":[[0,0,0,1],[1,0,3,0],[1,1,3,2],[1,3,3,4],[1,5,3,5],[1,6,3,7],[1,8,1,11],[2,8,3,9],[2,10,3,10],[2,11,3,11],[4,1,4,2],[4,3,4,4],[4,6,4,7],[4,8,4,9],[5,1,5,2],[5,3,5,4],[5,6,5,7],[5,8,5,9],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[9,1,9,2],[9,3,9,4],[9,6,9,7],[9,8,9,9],[10,1,10,2],[10,3,10,4],[10,6,10,7],[10,8,10,9],[11,1,11,2],[11,3,11,4],[11,6,11,7],[11,8,11,9],[12,1,12,2],[12,3,12,4],[12,6,12,7],[12,8,12,9],[13,1,13,2],[13,3,13,4],[13,6,13,7],[13,8,13,9],[14,1,14,2],[14,3,14,4],[14,6,14,7],[14,8,14,9],[15,1,15,2],[15,3,15,4],[15,6,15,7],[15,8,15,9],[16,1,16,2],[16,3,16,4],[16,6,16,7],[16,8,16,9],[17,1,17,2],[17,3,17,4],[17,6,17,7],[17,8,17,9],[18,1,18,2],[18,3,18,4],[18,6,18,7],[18,8,18,9],[19,1,19,2],[19,3,19,4],[19,6,19,7],[19,8,19,9],[20,1,20,2],[20,3,20,4],[20,6,20,7],[20,8,20,9],[21,1,21,2],[21,3,21,4],[21,6,21,7],[21,8,21,9],[22,1,22,2],[22,3,22,4],[22,6,22,7],[22,8,22,9],[23,1,23,2],[23,3,23,4],[23,6,23,7],[23,8,23,9],[24,1,24,2],[24,3,24,4],[24,6,24,7],[24,8,24,9],[25,0,25,9],[26,0,26,9]],"flags":["formulas_cached_only"]}
["附件三"]
["序号","项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","备注"]
[]
[null,"拆除工程"]
[1,"天棚面龙骨及饰面拆除 金属龙骨 石膏面",null,"1、名称：原轻钢龙骨石膏板吊顶拆除\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"10m2",2.517]
[2,"建筑垃圾外运",null,"1.名称：建筑垃圾装车、外运\n2.备注：运距自行考虑，满足建设单位、图纸设计及施工规范要求",null,"10m3",0.07551]
[null,"新建工程"]
[1,"石膏板天棚面层",null,"1、名称：石膏板天棚面层\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.2517]
[2,"轻钢龙骨石膏板",null,"1、名称：轻钢龙骨石膏板\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.2517]
[3,"石膏板棚面刷乳胶漆",null,"1、名称：石膏板棚面刷乳胶漆\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.2517]
[4,"棚面木梁",null,"1、名称：棚面木梁\n2、材质规格：榉木多层板200mm*70mm\n3、备注：满足建设单位、图纸设计及施工规范要求",null,"m",52.592]
[5,"墙面木柱",null,"1、名称：墙面木柱\n2、材质规格：榉木多层板100mm*100mm\n3、备注：满足建设单位、图纸设计及施工规范要求",null,"m",20.2]
[6,"棚面木梁、墙面木柱刷清漆",null,"1、名称：棚面木梁、墙面木柱刷清漆\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.364797]
[7,"铁艺连接件",null,"1、名称：铁艺连接件\n2、规格：具体尺寸详见图纸\n3、备注：满足建设单位、图纸设计及施工规范要求",null,"个",42]
[8,"墙饰面 面层 木质饰面板 墙面、墙裙",null,"1、名称：木饰面墙面\n2、材质规格：18mm厚桦木多层板\n3、做法：如现场不打木基层，安装方式则为粘胶固定\n4、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.252096]
[9,"吧台见面瓷砖铺贴",null,"1、名称：吧台见面瓷砖铺贴\n2、规格：200mm*400mm瓷砖\n3、做法：铺贴和填缝剂勾缝\n4、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.07216]
[10,"地柜",null,"1、名称：地柜\n2、规格：地柜门板厚度为18mm,柜体顶底侧层板均为18mm\n3、备注：满足建设单位、图纸设计及施工规范要求",null,"m",16.66]
[11,"地柜台面板 石英石",null,"1、名称：石英石台面\n2、规格：石英石厚度为40mm(15厚+25厚折边)\n3、备注：满足建设单位、图纸设计及施工规范要求",null,"m",16.66]
[12,"硅酸钙板涂料饰面",null,"1、名称：硅酸钙板涂料饰面\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.065205]
[13,"明管处不锈钢装饰",null,"1、名称：明管处不锈钢装饰\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"m",3]
[14,"室内亚克力发光字及logo",null,"1、名称：室内亚克力发光字及logo\n2、规格：具体尺寸详见图纸\n3、备注：含安装，满足建设单位、图纸设计及施工规范要求",null,"10个",0.5]
[15,"室外亚克力发光字及logo",null,"1、名称：室外亚克力发光字及logo\n2、规格：具体尺寸详见图纸\n3、备注：含骨架及安装，满足建设单位、图纸设计及施工规范要求",null,"10个",1]
[16,"立式功能牌匾",null,"1、名称：立式功能牌匾\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"个",2]
[17,"脚手架",null,"1、名称：脚手架\n2、备注：满足建设单位、图纸设计及施工规范要求",null,"100m2",0.228218]
["本页小计"]
["合   计"]