{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["扉-1 招标工程量清单扉页","表-08 分部分项工程和单价措施项目清单与计价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"扉-1 招标工程量清单扉页","index":0,"n_rows":11,"n_cols":7,"rows_kept":11,"merged":[[0,0,0,1],[0,2,0,4],[0,5,0,6],[1,0,1,1],[1,2,1,4],[1,5,1,6],[2,1,2,2],[2,4,2,5],[3,1,3,2],[3,4,3,5],[4,1,4,2],[4,4,4,5],[5,1,5,2],[5,4,5,5],[6,1,6,2],[6,4,6,5],[7,1,7,2],[7,4,7,5],[8,1,8,2],[8,4,8,5],[9,1,9,2],[9,4,9,5],[10,0,10,1],[10,2,10,4],[10,5,10,6]],"flags":["formulas_cached_only"]}
[null,null,"浑南国际产业园部分市政项目零散维修",null,null,"工程"]
[null,null,"招标工程量清单"]
[]
["招  标  人：",{"$nulls":3},"造 价咨询人："]
[null,"(单位盖章)",{"$nulls":4},"(单位资质专用章)"]
["法定代表人\n或其授权人：",{"$nulls":3},"法定代表人\n或其授权人："]
[null,"(签字或盖章)",{"$nulls":4},"(签字或盖章)"]
["编  制  人：",{"$nulls":3},"复  核  人："]
[null,"(造价人员签字盖专用章)",{"$nulls":4},"(造价工程师签字盖专用章)"]
["编 制 时 间：","    年   月   日",null,null,"复 核 时 间：",null,"    年   月   日"]
[{"$nulls":5},"扉—1"]

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表","index":1,"n_rows":329,"n_cols":14,"rows_kept":329,"merged":[[0,0,0,10],[0,11,0,13],[1,0,1,13],[2,0,2,5],[2,6,2,10],[2,11,2,13],[3,10,3,13],[6,1,6,2],[6,3,6,4],[6,5,6,6],[6,8,6,9],[6,10,6,11],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,8,7,9],[7,10,7,11],[8,1,8,2],[8,3,8,4],[8,5,8,6],[8,8,8,9],[8,10,8,11],[9,1,9,2],[9,3,9,4],[9,5,9,6],[9,8,9,9],[9,10,9,11],[10,1,10,2],[10,3,10,4],[10,5,10,6],[10,8,10,9],[10,10,10,11],[11,1,11,2],[11,3,11,4],[11,5,11,6],[11,8,11,9],[11,10,11,11],[12,1,12,2],[12,3,12,4],[12,5,12,6],[12,8,12,9],[12,10,12,11],[13,1,13,2],[13,3,13,4],[13,5,13,6],[13,8,13,9],[13,10,13,11],[14,1,14,2],[14,3,14,4],[14,5,14,6],[14,8,14,9],[14,10,14,11],[15,1,15,2],[15,3,15,4],[15,5,15,6],[15,8,15,9],[15,10,15,11],[16,1,16,2],[16,3,16,4],[16,5,16,6],[16,8,16,9],[16,10,16,11],[17,1,17,2],[17,3,17,4],[17,5,17,6],[17,8,17,9],[17,10,17,11],[18,1,18,2],[18,3,18,4],[18,5,18,6],[18,8,18,9],[18,10,18,11],[19,1,19,2],[19,3,19,4],[19,5,19,6],[19,8,19,9],[19,10,19,11],[20,0,20,9],[20,10,20,11],[21,0,21,1],[21,2,21,3],[21,4,21,5],[21,6,21,8],[21,9,21,10],[21,11,21,13],[22,0,22,10],[22,11,22,13],[23,0,23,13],[24,0,24,5],[24,6,24,10],[24,11,24,13],[25,10,25,13],[28,1,28,2],[28,3,28,4],[28,5,28,6],[28,8,28,9],[28,10,28,11],[29,1,29,2],[29,3,29,4],[29,5,29,6],[29,8,29,9],[29,10,29,11],[30,1,30,2],[30,3,30,4],[30,5,30,6],[30,8,30,9],[30,10,30,11],[31,1,31,2],[31,3,31,4],[31,5,31,6],[31,8,31,9],[31,10,31,11],[32,1,32,2],[32,3,32,4],[32,5,32,6],[32,8,32,9],[32,10,32,11],[33,1,33,2],[33,3,33,4],[33,5,33,6],[33,8,33,9],[33,10,33,11],[34,1,34,2],[34,3,34,4],[34,5,34,6],[34,8,34,9],[34,10,34,11],[35,1,35,2],[35,3,35,4],[35,5,35,6],[35,8,35,9],[35,10,35,11],[36,1,36,2],[36,3,36,4],[36,5,36,6],[36,8,36,9],[36,10,36,11],[37,1,37,2],[37,3,37,4],[37,5,37,6],[37,8,37,9],[37,10,37,11],[38,1,38,2],[38,3,38,4],[38,5,38,6],[38,8,38,9],[38,10,38,11],[39,1,39,2],[39,3,39,4],[39,5,39,6],[39,8,39,9],[39,10,39,11],[40,1,40,2],[40,3,40,4],[40,5,40,6],[40,8,40,9],[40,10,40,11],[41,0,41,9],[41,10,41,11],[42,0,42,1],[42,2,42,3],[42,4,42,5],[42,6,42,8],[42,9,42,10],[42,11,42,13],[43,0,43,10],[43,11,43,13],[44,0,44,13],[45,0,45,5],[45,6,45,10],[45,11,45,13],[46,10,46,13],[49,1,49,2],[49,3,49,4],[49,5,49,6],[49,8,49,9],[49,10,49,11],[50,1,50,2],[50,3,50,4],[50,5,50,6],[50,8,50,9],[50,10,50,11],[51,1,51,2],[51,3,51,4],[51,5,51,6],[51,8,51,9],[51,10,51,11],[52,1,52,2],[52,3,52,4],[52,5,52,6],[52,8,52,9],[52,10,52,11],[53,1,53,2],[53,3,53,4],[53,5,53,6],[53,8,53,9],[53,10,53,11],[54,1,54,2],[54,3,54,4],[54,5,54,6],[54,8,54,9],[54,10,54,11],[55,1,55,2],[55,3,55,4],[55,5,55,6],[55,8,55,9],[55,10,55,11],[56,1,56,2],[56,3,56,4],[56,5,56,6],[56,8,56,9],[56,10,56,11],[57,1,57,2],[57,3,57,4],[57,5,57,6],[57,8,57,9],[57,10,57,11],[58,1,58,2],[58,3,58,4],[58,5,58,6],[58,8,58,9],[58,10,58,11],[59,1,59,2],[59,3,59,4],[59,5,59,6],[59,8,59,9],[59,10,59,11],[60,1,60,2],[60,3,60,4],[60,5,60,6],[60,8,60,9],[60,10,60,11],[61,1,61,2],[61,3,61,4],[61,5,61,6],[61,8,61,9],[61,10,61,11],[62,0,62,9],[62,10,62,11],[63,0,63,1],[63,2,63,3],[63,4,63,5],[63,6,63,8],[63,9,63,10],[63,11,63,13],[64,0,64,10],[64,11,64,13],[65,0,65,13],[66,0,66,5],[66,6,66,10],[66,11,66,13],[67,10,67,13],[70,1,70,2],[70,3,70,4],[70,5,70,6],[70,8,70,9],[70,10,70,11],[71,1,71,2],[71,3,71,4],[71,5,71,6],[71,8,71,9],[71,10,71,11],[72,1,72,2],[72,3,72,4],[72,5,72,6],[72,8,72,9],[72,10,72,11],[73,1,73,2],[73,3,73,4],[73,5,73,6],[73,8,73,9],[73,10,73,11],[74,1,74,2],[74,3,74,4],[74,5,74,6],[74,8,74,9],[74,10,74,11],[75,1,75,2],[75,3,75,4],[75,5,75,6],[75,8,75,9],[75,10,75,11],[76,1,76,2],[76,3,76,4],[76,5,76,6],[76,8,76,9],[76,10,76,11],[77,1,77,2],[77,3,77,4],[77,5,77,6],[77,8,77,9],[77,10,77,11],[78,1,78,2],[78,3,78,4],[78,5,78,6],[78,8,78,9],[78,10,78,11],[79,1,79,2],[79,3,79,4],[79,5,79,6],[79,8,79,9],[79,10,79,11],[80,1,80,2],[80,3,80,4],[80,5,80,6],[80,8,80,9],[80,10,80,11],[81,1,81,2],[81,3,81,4],[81,5,81,6],[81,8,81,9],[81,10,81,11],[82,1,82,2],[82,3,82,4],[82,5,82,6],[82,8,82,9],[82,10,82,11],[83,0,83,9],[83,10,83,11],[84,0,84,1],[84,2,84,3],[84,4,84,5],[84,6,84,8],[84,9,84,10],[84,11,84,13],[85,0,85,10],[85,11,85,13],[86,0,86,13],[87,0,87,5],[87,6,87,10],[87,11,87,13],[88,10,88,13],[91,1,91,2],[91,3,91,4],[91,5,91,6],[91,8,91,9],[91,10,91,11],[92,1,92,2],[92,3,92,4],[92,5,92,6],[92,8,92,9],[92,10,92,11],[93,1,93,2],[93,3,93,4],[93,5,93,6],[93,8,93,9],[93,10,93,11],[94,1,94,2],[94,3,94,4],[94,5,94,6],[94,8,94,9],[94,10,94,11],[95,1,95,2],[95,3,95,4],[95,5,95,6],[95,8,95,9],[95,10,95,11],[96,1,96,2],[96,3,96,4],[96,5,96,6],[96,8,96,9],[96,10,96,11],[97,1,97,2],[97,3,97,4],[97,5,97,6],[97,8,97,9],[97,10,97,11],[98,1,98,2],[98,3,98,4],[98,5,98,6],[98,8,98,9],[98,10,98,11],[99,1,99,2],[99,3,99,4],[99,5,99,6],[99,8,99,9],[99,10,99,11],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,8,100,9],[100,10,100,11],[101,1,101,2],[101,3,101,4],[101,5,101,6],[101,8,101,9],[101,10,101,11],[102,1,102,2],[102,3,102,4],[102,5,102,6],[102,8,102,9],[102,10,102,11],[103,1,103,2],[103,3,103,4],[103,5,103,6],[103,8,103,9],[103,10,103,11],[104,1,104,2],[104,3,104,4],[104,5,104,6],[104,8,104,9],[104,10,104,11],[105,0,105,9],[105,10,105,11],[106,0,106,1],[106,2,106,3],[106,4,106,5],[106,6,106,8],[106,9,106,10],[106,11,106,13],[107,0,107,10],[107,11,107,13],[108,0,108,13],[109,0,109,5],[109,6,109,10],[109,11,109,13],[110,10,110,13],[113,1,113,2],[113,3,113,4],[113,5,113,6],[113,8,113,9],[113,10,113,11],[114,1,114,2],[114,3,114,4],[114,5,114,6],[114,8,114,9],[114,10,114,11],[115,1,115,2],[115,3,115,4],[115,5,115,6],[115,8,115,9],[115,10,115,11],[116,1,116,2],[116,3,116,4],[116,5,116,6],[116,8,116,9],[116,10,116,11],[117,1,117,2],[117,3,117,4],[117,5,117,6],[117,8,117,9],[117,10,117,11],[118,1,118,2],[118,3,118,4],[118,5,118,6],[118,8,118,9],[118,10,118,11],[119,1,119,2],[119,3,119,4],[119,5,119,6],[119,8,119,9],[119,10,119,11],[120,1,120,2],[120,3,120,4],[120,5,120,6],[120,8,120,9],[120,10,120,11],[121,1,121,2],[121,3,121,4],[121,5,121,6],[121,8,121,9],[121,10,121,11],[122,1,122,2],[122,3,122,4],[122,5,122,6],[122,8,122,9],[122,10,122,11],[123,1,123,2],[123,3,123,4],[123,5,123,6],[123,8,123,9],[123,10,123,11],[124,1,124,2],[124,3,124,4],[124,5,124,6],[124,8,124,9],[124,10,124,11],[125,0,125,9],[125,10,125,11],[126,0,126,1],[126,2,126,3],[126,4,126,5],[126,6,126,8],[126,9,126,10],[126,11,126,13],[127,0,127,10],[127,11,127,13],[128,0,128,13],[129,0,129,5],[129,6,129,10],[129,11,129,13],[130,10,130,13],[133,1,133,2],[133,3,133,4],[133,5,133,6],[133,8,133,9],[133,10,133,11],[134,1,134,2],[134,3,134,4],[134,5,134,6],[134,8,134,9],[134,10,134,11],[135,1,135,2],[135,3,135,4],[135,5,135,6],[135,8,135,9],[135,10,135,11],[136,1,136,2],[136,3,136,4],[136,5,136,6],[136,8,136,9],[136,10,136,11],[137,1,137,2],[137,3,137,4],[137,5,137,6],[137,8,137,9],[137,10,137,11],[138,1,138,2],[138,3,138,4],[138,5,138,6],[138,8,138,9],[138,10,138,11],[139,1,139,2],[139,3,139,4],[139,5,139,6],[139,8,139,9],[139,10,139,11],[140,1,140,2],[140,3,140,4],[140,5,140,6],[140,8,140,9],[140,10,140,11],[141,1,141,2],[141,3,141,4],[141,5,141,6],[141,8,141,9],[141,10,141,11],[142,1,142,2],[142,3,142,4],[142,5,142,6],[142,8,142,9],[142,10,142,11],[143,1,143,2],[143,3,143,4],[143,5,143,6],[143,8,143,9],[143,10,143,11],[144,1,144,2],[144,3,144,4],[144,5,144,6],[144,8,144,9],[144,10,144,11],[145,1,145,2],[145,3,145,4],[145,5,145,6],[145,8,145,9],[145,10,145,11],[146,1,146,2],[146,3,146,4],[146,5,146,6],[146,8,146,9],[146,10,146,11],[147,1,147,2],[147,3,147,4],[147,5,147,6],[147,8,147,9],[147,10,147,11],[148,0,148,9],[148,10,148,11],[149,0,149,1],[149,2,149,3],[149,4,149,5],[149,6,149,8],[149,9,149,10],[149,11,149,13],[150,0,150,10],[150,11,150,13],[151,0,151,13],[152,0,152,5],[152,6,152,10],[152,11,152,13],[153,10,153,13],[156,1,156,2],[156,3,156,4],[156,5,156,6],[156,8,156,9],[156,10,156,11],[157,1,157,2],[157,3,157,4],[157,5,157,6],[157,8,157,9],[157,10,157,11],[158,1,158,2],[158,3,158,4],[158,5,158,6],[158,8,158,9],[158,10,158,11],[159,1,159,2],[159,3,159,4],[159,5,159,6],[159,8,159,9],[159,10,159,11],[160,1,160,2],[160,3,160,4],[160,5,160,6],[160,8,160,9],[160,10,160,11],[161,1,161,2],[161,3,161,4],[161,5,161,6],[161,8,161,9],[161,10,161,11],[162,1,162,2],[162,3,162,4],[162,5,162,6],[162,8,162,9],[162,10,162,11],[163,1,163,2],[163,3,163,4],[163,5,163,6],[163,8,163,9],[163,10,163,11],[164,1,164,2],[164,3,164,4],[164,5,164,6],[164,8,164,9],[164,10,164,11],[165,1,165,2],[165,3,165,4],[165,5,165,6],[165,8,165,9],[165,10,165,11],[166,1,166,2],[166,3,166,4],[166,5,166,6],[166,8,166,9],[166,10,166,11],[167,1,167,2],[167,3,167,4],[167,5,167,6],[167,8,167,9],[167,10,167,11],[168,1,168,2],[168,3,168,4],[168,5,168,6],[168,8,168,9],[168,10,168,11],[169,1,169,2],[169,3,169,4],[169,5,169,6],[169,8,169,9],[169,10,169,11],[170,0,170,9],[170,10,170,11],[171,0,171,1],[171,2,171,3],[171,4,171,5],[171,6,171,8],[171,9,171,10],[171,11,171,13],[172,0,172,10],[172,11,172,13],[173,0,173,13],[174,0,174,5],[174,6,174,10],[174,11,174,13],[175,10,175,13],[178,1,178,2],[178,3,178,4],[178,5,178,6],[178,8,178,9],[178,10,178,11],[179,1,179,2],[179,3,179,4],[179,5,179,6],[179,8,179,9],[179,10,179,11],[180,1,180,2],[180,3,180,4],[180,5,180,6],[180,8,180,9],[180,10,180,11],[181,1,181,2],[181,3,181,4],[181,5,181,6],[181,8,181,9],[181,10,181,11],[182,1,182,2],[182,3,182,4],[182,5,182,6],[182,8,182,9],[182,10,182,11],[183,1,183,2],[183,3,183,4],[183,5,183,6],[183,8,183,9],[183,10,183,11],[184,1,184,2],[184,3,184,4],[184,5,184,6],[184,8,184,9],[184,10,184,11],[185,1,185,2],[185,3,185,4],[185,5,185,6],[185,8,185,9],[185,10,185,11],[186,1,186,2],[186,3,186,4],[186,5,186,6],[186,8,186,9],[186,10,186,11],[187,1,187,2],[187,3,187,4],[187,5,187,6],[187,8,187,9],[187,10,187,11],[188,1,188,2],[188,3,188,4],[188,5,188,6],[188,8,188,9],[188,10,188,11],[189,1,189,2],[189,3,189,4],[189,5,189,6],[189,8,189,9],[189,10,189,11],[190,1,190,2],[190,3,190,4],[190,5,190,6],[190,8,190,9],[190,10,190,11],[191,0,191,9],[191,10,191,11],[192,0,192,1],[192,2,192,3],[192,4,192,5],[192,6,192,8],[192,9,192,10],[192,11,192,13],[193,0,193,10],[193,11,193,13],[194,0,194,13],[195,0,195,5],[195,6,195,10],[195,11,195,13],[196,10,196,13],[199,1,199,2],[199,3,199,4],[199,5,199,6],[199,8,199,9],[199,10,199,11],[200,1,200,2],[200,3,200,4],[200,5,200,6],[200,8,200,9],[200,10,200,11],[201,1,201,2],[201,3,201,4],[201,5,201,6],[201,8,201,9],[201,10,201,11],[202,1,202,2],[202,3,202,4],[202,5,202,6],[202,8,202,9],[202,10,202,11],[203,1,203,2],[203,3,203,4],[203,5,203,6],[203,8,203,9],[203,10,203,11],[204,1,204,2],[204,3,204,4],[204,5,204,6],[204,8,204,9],[204,10,204,11],[205,1,205,2],[205,3,205,4],[205,5,205,6],[205,8,205,9],[205,10,205,11],[206,1,206,2],[206,3,206,4],[206,5,206,6],[206,8,206,9],[206,10,206,11],[207,1,207,2],[207,3,207,4],[207,5,207,6],[207,8,207,9],[207,10,207,11],[208,1,208,2],[208,3,208,4],[208,5,208,6],[208,8,208,9],[208,10,208,11],[209,1,209,2],[209,3,209,4],[209,5,209,6],[209,8,209,9],[209,10,209,11],[210,1,210,2],[210,3,210,4],[210,5,210,6],[210,8,210,9],[210,10,210,11],[211,1,211,2],[211,3,211,4],[211,5,211,6],[211,8,211,9],[211,10,211,11],[212,0,212,9],[212,10,212,11],[213,0,213,1],[213,2,213,3],[213,4,213,5],[213,6,213,8],[213,9,213,10],[213,11,213,13],[214,0,214,10],[214,11,214,13],[215,0,215,13],[216,0,216,5],[216,6,216,10],[216,11,216,13],[217,10,217,13],[220,1,220,2],[220,3,220,4],[220,5,220,6],[220,8,220,9],[220,10,220,11],[221,1,221,2],[221,3,221,4],[221,5,221,6],[221,8,221,9],[221,10,221,11],[222,1,222,2],[222,3,222,4],[222,5,222,6],[222,8,222,9],[222,10,222,11],[223,1,223,2],[223,3,223,4],[223,5,223,6],[223,8,223,9],[223,10,223,11],[224,1,224,2],[224,3,224,4],[224,5,224,6],[224,8,224,9],[224,10,224,11],[225,1,225,2],[225,3,225,4],[225,5,225,6],[225,8,225,9],[225,10,225,11],[226,1,226,2],[226,3,226,4],[226,5,226,6],[226,8,226,9],[226,10,226,11],[227,1,227,2],[227,3,227,4],[227,5,227,6],[227,8,227,9],[227,10,227,11],[228,1,228,2],[228,3,228,4],[228,5,228,6],[228,8,228,9],[228,10,228,11],[229,1,229,2],[229,3,229,4],[229,5,229,6],[229,8,229,9],[229,10,229,11],[230,1,230,2],[230,3,230,4],[230,5,230,6],[230,8,230,9],[230,10,230,11],[231,1,231,2],[231,3,231,4],[231,5,231,6],[231,8,231,9],[231,10,231,11],[232,1,232,2],[232,3,232,4],[232,5,232,6],[232,8,232,9],[232,10,232,11],[233,1,233,2],[233,3,233,4],[233,5,233,6],[233,8,233,9],[233,10,233,11],[234,1,234,2],[234,3,234,4],[234,5,234,6],[234,8,234,9],[234,10,234,11],[235,0,235,9],[235,10,235,11],[236,0,236,1],[236,2,236,3],[236,4,236,5],[236,6,236,8],[236,9,236,10],[236,11,236,13],[237,0,237,10],[237,11,237,13],[238,0,238,13],[239,0,239,5],[239,6,239,10],[239,11,239,13],[240,10,240,13],[243,1,243,2],[243,3,243,4],[243,5,243,6],[243,8,243,9],[243,10,243,11],[244,1,244,2],[244,3,244,4],[244,5,244,6],[244,8,244,9],[244,10,244,11],[245,1,245,2],[245,3,245,4],[245,5,245,6],[245,8,245,9],[245,10,245,11],[246,1,246,2],[246,3,246,4],[246,5,246,6],[246,8,246,9],[246,10,246,11],[247,1,247,2],[247,3,247,4],[247,5,247,6],[247,8,247,9],[247,10,247,11],[248,1,248,2],[248,3,248,4],[248,5,248,6],[248,8,248,9],[248,10,248,11],[249,1,249,2],[249,3,249,4],[249,5,249,6],[249,8,249,9],[249,10,249,11],[250,1,250,2],[250,3,250,4],[250,5,250,6],[250,8,250,9],[250,10,250,11],[251,1,251,2],[251,3,251,4],[251,5,251,6],[251,8,251,9],[251,10,251,11],[252,1,252,2],[252,3,252,4],[252,5,252,6],[252,8,252,9],[252,10,252,11],[253,1,253,2],[253,3,253,4],[253,5,253,6],[253,8,253,9],[253,10,253,11],[254,1,254,2],[254,3,254,4],[254,5,254,6],[254,8,254,9],[254,10,254,11],[255,1,255,2],[255,3,255,4],[255,5,255,6],[255,8,255,9],[255,10,255,11],[256,1,256,2],[256,3,256,4],[256,5,256,6],[256,8,256,9],[256,10,256,11],[257,1,257,2],[257,3,257,4],[257,5,257,6],[257,8,257,9],[257,10,257,11],[258,0,258,9],[258,10,258,11],[259,0,259,1],[259,2,259,3],[259,4,259,5],[259,6,259,8],[259,9,259,10],[259,11,259,13]],"merged_total":1387,"flags":["formulas_cached_only","merged_cut"]}
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  1  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":3},"园区边石、篦子修缮"]
[1,"040204004034",null,"拆除边石",null,"1.名称：拆除旧边石\n2.满足图纸及相关规范设计要求",null,"100m",1.35]
[2,"04001",null,"边石打磨",null,"1.名称：旧边石打磨\n2.满足图纸及相关规范设计要求",null,"m",115]
[3,"040204004035",null,"打磨完边石安装",null,"1.名称：旧边石安装\n2.满足图纸及相关规范设计要求",null,"100m",1.15]
[4,"040204004036",null,"新安装边石150*180*990",null,"1.名称：新边石安装\n2.做法：150*180*990边石\n3.满足图纸及相关规范设计要求",null,"100m",0.2]
[5,"04002",null,"更换雨水篦子",null,"1.名称：更换雨水篦子\n2.做法：规格详见图纸\n3.满足图纸及相关规范设计要求",null,"个",44]
[6,"040204004033",null,"更换雨水篦子拆安边石",null,"1.名称：更换雨水篦子拆安边石\n2.做法：规格详见图纸\n3.满足图纸及相关规范设计要求",null,"100m",0.44]
[7,"040204004026",null,"调整下沉边石（边石利旧）",null,"1.名称：调整下沉边石（利旧）\n2.满足图纸及相关规范设计要求",null,"100m",2.18]
[8,"040204004003",null,"人工铺装垫层 预拌混凝土",null,"1.名称：混凝土垫层\n2.部位：边上靠背垫层\n3.做法：C15预拌混凝土\n4.满足图纸及相关规范设计要求",null,"10m3",0.5295]
[{"$nulls":3},"3G门前维修"]
[1,"041001001003",null,"拆除混凝土类路面层 机械拆除(无筋) 厚15cm内",null,"1.名称：拆除混凝土地面（300mm厚）\n2.满足图纸及相关规范设计要求",null,"100m2",0.18666]
[2,"040105008004",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.0056]
[3,"040105009006",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.0056]
[4,"040204004027",null,"混凝土200mm厚c20",null,"1.名称：混凝土地面\n2.做法：C20混凝土 ",null,"10m3",0.37332]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  2  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":5},"200mm厚\n3.满足图纸及相关规范设计要求"]
[5,"040901001017",null,"现浇构件钢筋 带肋钢筋 直径14mm",null,"1.规格：三级钢筋14\n2.钢筋制作、运输、绑扎、安装\n3.满足图纸及相关规范设计要求",null,"t",0.232459]
[6,"040203003011",null,"透层 半刚性基层 乳化沥青 0.7kg/m2",null,"1.透层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.018666]
[7,"040203003012",null,"黏(粘)层 沥青层 乳化沥青 0.3kg/m2",null,"1.黏层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.018666]
[8,"040203006031",null,"沥青混凝土路面 中粒式 机械摊铺50m2以内 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.18666]
[9,"040203006033",null,"沥青混凝土路面 细粒式 机械摊铺50m2以内 厚度4cm",null,"1.4cm厚细粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.18666]
[10,"040204011006",null,"沥青混凝土 自卸汽车运输 运距15km以内",null,"1.沥青混凝土运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.045746]
[{"$nulls":3},"14C东南侧雨污混排维修"]
[1,"040104003007",null,"反铲挖掘机挖槽坑土方 一、二类土",null,"1.名称：机械挖土\n2.土壤类别：一、二类土\n3.满足图纸及规范设计要求",null,"1000m3",0.0384]
[2,"040104006001",null,"挖掘机装土方 挖掘机1m3",null,"1.名称：土方装车\n2.满足图纸及规范设计要求",null,"1000m3",0.0384]
[3,"040104006009",null,"自卸汽车运土方 运距≤1km",null,"1.名称：土方外运\n2.做法：运距10km\n3.满足设计及相关规范要求",null,"1000m3",0.0384]
[4,"040103003002",null,"直埋管沟回填 砂",null,"1.名称：回填砂\n2.满足设计及相关规范要求",null,"10m3",3.84]
[5,"040204004028",null,"混凝土封堵污水",null,"1.名称：混凝土堵管",null,"10m3",0.003533]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  3  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":3},"管",null,"2.做法：C15混凝土\n3.满足设计及相关规范要求"]
[6,"040203014004",null,"切割机切割路面 沥青混凝土路面 厚度10cm以内",null,"1.切割路面\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m",0.36]
[7,"041001001008",null,"拆除沥青柏油类路面层 小型机械拆除 厚10cm厚",null,"1.沥青路面拆除\n2.满足图纸及规范设计要求",null,"100m2",0.8]
[8,"041001014008",null,"液压岩石破碎机破碎砼及钢筋砼 沥青混凝土面层、半刚性材料",null,"1.名称：破碎地面\n2.满足图纸及规范设计要求",null,"1000m3",0.024]
[9,"040105008005",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.032]
[10,"040105009007",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.032]
[11,"040202001004",null,"路床整形 路床碾压检验",null,"1.路床碾压\n2.满足图纸及规范设计要求",null,"100m2",0.8]
[12,"040202032012",null,"厂拌水泥稳定砂砾(50m2以外) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.8]
[13,"040202036007",null,"基层养生 塑料膜养生",null,"1.基层养生\n2.满足图纸及规范设计要求",null,"100m2",0.8]
[14,"040203003013",null,"透层 半刚性基层 乳化沥青 0.7kg/m2",null,"1.透层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.08]
[15,"040203003014",null,"黏(粘)层 沥青层 乳化沥青 0.3kg/m2",null,"1.黏层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.08]
[16,"040203006034",null,"沥青混凝土路面 中粒式 机械摊铺50m2以外 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.8]
[17,"040203006036",null,"沥青混凝土路面 细粒式 机械摊",null,"1.4cm厚细粒式沥青混凝土",null,"100m2",0.8]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  4  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":3},"铺50m2以外 厚度4cm",null,"2.部位：沥青路面\n3.满足图纸及相关规范设计要求"]
[18,"040204010006",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.601832]
[19,"040204011007",null,"沥青混凝土 自卸汽车运输 运距15km以内",null,"1.沥青混凝土运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.196019]
[20,"040204006024",null,"检查井、窨井 升高30cm",null,"1.调整检查井\n2.部位：沥青路面上的检查井调整高度同路面\n3.满足图纸及相关规范设计要求",null,"座",2]
[{"$nulls":3},"24H厂房东侧室外消防管线渗漏维修"]
[1,"040104003043",null,"反铲挖掘机挖槽坑土方 一、二类土",null,"1.名称：机械挖土\n2.土壤类别：一、二类土\n3.满足图纸及规范设计要求",null,"1000m3",0.1008]
[2,"040104006013",null,"挖掘机装土方 挖掘机1m3",null,"1.名称：土方装车\n2.满足图纸及规范设计要求",null,"1000m3",0.1008]
[3,"040104006014",null,"自卸汽车运土方 运距≤1km",null,"1.名称：土方外运\n2.做法：运距10km\n3.满足设计及相关规范要求",null,"1000m3",0.1008]
[4,"040103003004",null,"直埋管沟回填 砂",null,"1.名称：回填砂\n2.满足设计及相关规范要求",null,"10m3",8.011584]
[5,"041001007002",null,"拆除砖石构筑物 砖砌检查井 深3m以内",null,"1.名称：拆除原检查井\n2.满足设计及相关规范要求",null,"10m3",0.79032]
[6,"040504001043",null,"砖砌水井 井室净尺寸(长*宽*高)2.5*2.3*1.94m",null,"1.名称：砌筑检查井\n2.满足设计及相关规范要求",null,"座",1]
[7,"040502020021",null,"给水附件安装 铸铁穿墙管安装 公称直径法兰DN200mm以内",null,"1.满足设计及相关规范要求",null,"个",1]
[8,"040602031001",null,"铸铁圆闸门 直径200mm",null,"1.名称：铸铁圆闸门\n2.满足设计及相关规范要求",null,"座",1]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  5  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[9,"041001002007",null,"拆除人行道 荷兰砖",null,"1.名称：拆除荷兰砖\n2.满足设计及相关规范要求",null,"100m2",1.3325]
[10,"041001014011",null,"拆除原有找平层及水稳层",null,"1.名称：破碎地面\n2.满足设计及相关规范要求",null,"1000m3",0.046638]
[11,"040105008007",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.046638]
[12,"040105009009",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.046638]
[13,"040204001002",null,"人行道整形碾压",null,"1.名称：路床碾压\n2.满足图纸及规范设计要求",null,"100m2",1.3325]
[14,"040204002044",null,"人行道块料铺设 水泥砂浆 规格20*10*6cm(利旧70%)",null,"1.名称：步道砖铺设\n2.做法：预制砼彩色步砖200*100*60(70%利旧)\n3.满足图纸及规范设计要求",null,"100m2",1.3325]
[15,"040202032017",null,"厂拌水泥稳定砂砾(50m2以外) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",1.2325]
[16,"040204010010",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.927197]
[{"$nulls":3},"24H厂房路面维修"]
[1,"040203014003",null,"切割机切割路面 沥青混凝土路面 厚度10cm以内",null,"1.切割路面\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m",0.38]
[2,"041001001007",null,"拆除沥青柏油类路面层 小型机械拆除 厚10cm厚",null,"1.沥青路面拆除\n2.满足图纸及规范设计要求",null,"100m2",0.9]
[3,"041001014007",null,"液压岩石破碎机破碎砼及钢筋砼 沥青混凝土面层、半刚性材料",null,"1.名称：破碎地面\n2.满足设计及相关规范要求",null,"1000m3",0.027]
[4,"040105008003",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.036]
[5,"040105009005",null,"运石渣 运距",null,"1.机械运石渣",null,"1000m3",0.036]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  6  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":3},"10km",null,"2.满足图纸及规范设计要求"]
[6,"040202001003",null,"路床整形 路床碾压检验",null,"1.名称：路床碾压\n2.满足图纸及规范设计要求",null,"100m2",0.9]
[7,"040202032010",null,"厂拌水泥稳定砂砾(50m2以外) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.6]
[8,"040202032011",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.3]
[9,"040202036006",null,"基层养生 塑料膜养生",null,"1.基层养生\n2.满足图纸及规范设计要求",null,"100m2",0.9]
[10,"040203003009",null,"透层 半刚性基层 乳化沥青 0.7kg/m2",null,"1.透层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.09]
[11,"040203003010",null,"黏(粘)层 沥青层 乳化沥青 0.3kg/m2",null,"1.黏层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.09]
[12,"040203006026",null,"沥青混凝土路面 中粒式 机械摊铺50m2以外 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.6]
[13,"040203006028",null,"沥青混凝土路面 中粒式 机械摊铺50m2以内 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.3]
[14,"040203006027",null,"沥青混凝土路面 细粒式 机械摊铺50m2以外 厚度4cm",null,"1.4cm厚细粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.6]
[15,"040203006029",null,"沥青混凝土路面 细粒式 机械摊铺50m2以内 厚度4cm",null,"1.4cm厚细粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.3]
[16,"040204010005",null,"水泥稳定粒料 ",null,"1.水稳运输",null,"100t",0.677061]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  7  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":3},"自卸汽车运输 运距15km以内",null,"2.部位：沥青路面\n3.满足图纸及相关规范设计要求"]
[17,"040204011005",null,"沥青混凝土 自卸汽车运输 运距15km以内",null,"1.沥青混凝土运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.220522]
[18,"041105002010",null,"特、大型机械进出场 压路机",null,"1.压路机进出场\n2.满足图纸及规范设计要求",null,"台次",1]
[19,"041105002001",null,"特、大型机械进出场 履带式挖掘机进出场费 1m3以内",null,"1.履带式挖掘机进出场\n2.满足图纸及规范设计要求",null,"台次",1]
[{"$nulls":3},"9B厂房北侧路面维修"]
[1,"040104003044",null,"反铲挖掘机挖槽坑土方 一、二类土",null,"1.名称：机械挖土\n2.土壤类别：一、二类土\n3.满足图纸及规范设计要求",null,"1000m3",0.077]
[2,"040104006015",null,"挖掘机装土方 挖掘机1m3",{"$nulls":3},"1000m3",0.077]
[3,"040104006016",null,"自卸汽车运土方 运距≤1km",{"$nulls":3},"1000m3",0.077]
[4,"040201022012",null,"垫层铺筑 砂",{"$nulls":3},"10m3",6.3]
[5,"040204004029",null,"混凝土封堵污水管",{"$nulls":3},"10m3",0.05652]
[6,"040203014005",null,"切割机切割路面 沥青混凝土路面 厚度10cm以内",null,"1.切割路面\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m",0.24]
[7,"041001001009",null,"拆除沥青柏油类路面层 小型机械拆除 厚10cm厚",null,"1.沥青路面拆除\n2.满足图纸及规范设计要求",null,"100m2",0.35]
[8,"041001014009",null,"液压岩石破碎机破碎砼及钢筋砼 沥青混凝土面层、半刚性材料",{"$nulls":3},"1000m3",0.0105]
[9,"040202001005",null,"路床整形 路床碾压检验",null,"1.路床碾压\n2.满足图纸及规范设计要求",null,"100m2",0.35]
[10,"040202032014",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设",null,"100m2",0.35]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  8  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":5},"计要求"]
[11,"040202036008",null,"基层养生 塑料膜养生",null,"1.基层养生\n2.满足图纸及规范设计要求",null,"100m2",0.35]
[12,"040203003015",null,"透层 半刚性基层 乳化沥青 0.7kg/m2",null,"1.透层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.035]
[13,"040203003016",null,"黏(粘)层 沥青层 乳化沥青 0.3kg/m2",null,"1.黏层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.035]
[14,"040203006038",null,"沥青混凝土路面 中粒式 机械摊铺50m2以内 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.35]
[15,"040203006040",null,"沥青混凝土路面 细粒式 机械摊铺50m2以内 厚度4cm",null,"1.4cm厚细粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.35]
[16,"040204010007",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.263302]
[17,"040204011008",null,"沥青混凝土 自卸汽车运输 运距15km以内",null,"1.沥青混凝土运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.085758]
[18,"040204004032",null,"混凝土封堵污水管",{"$nulls":3},"10m3",0.11304]
[{"$nulls":3},"15D厂房开一个车行路口"]
[1,"040101003012",null,"人工挖基坑土方 一、二类土深度在2m以内",null,"1.名称：人工挖土\n2.土壤类别：一、二类土\n3.满足图纸及规范设计要求",null,"100m3",0.0726]
[2,"040104006017",null,"挖掘机装土方 挖掘机1m3",null,"1.名称：土方装车\n2.满足图纸及规范设计要求",null,"1000m3",0.00726]
[3,"040104006018",null,"自卸汽车运土方 运距≤1km",null,"1.名称：土方外运\n2.做法：运距10km\n3.满足设计及相关规范要求",null,"1000m3",0.00726]
[4,"040202001006",null,"路床整形 路床碾压检验",null,"1.路床碾压\n2.满足图纸及规范设计要",null,"100m2",0.1815]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  9  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":5},"求"]
[5,"040202032015",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.1815]
[6,"040202036009",null,"基层养生 塑料膜养生",null,"1.基层养生\n2.满足图纸及规范设计要求",null,"100m2",0.1815]
[7,"040203003017",null,"透层 半刚性基层 乳化沥青 0.7kg/m2",null,"1.透层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.01815]
[8,"040203003018",null,"黏(粘)层 沥青层 乳化沥青 0.3kg/m2",null,"1.黏层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.01815]
[9,"040203006041",null,"沥青混凝土路面 中粒式 机械摊铺50m2以内 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.1815]
[10,"040203006042",null,"沥青混凝土路面 细粒式 机械摊铺50m2以内 厚度4cm",null,"1.4cm厚细粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.1815]
[11,"040204010008",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.136541]
[12,"040204011009",null,"沥青混凝土 自卸汽车运输 运距15km以内",null,"1.沥青混凝土运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.044472]
[13,"040204004030",null,"拆除边石",null,"1.名称：拆除边石\n2.满足图纸及相关规范设计要求",null,"100m",0.11]
[14,"040204004031",null,"安装边石（边石利旧）",null,"1.名称：边石安装\n2.做法：边石利旧\n3.满足图纸及相关规范设计要求",null,"100m",0.066]
[{"$nulls":3},"水泵房"]
[1,"041001002001",null,"拆除人行道 荷兰砖",null,"1.名称：拆除荷兰砖\n2.满足设计及相关规范要求",null,"100m2",1.5725]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  10  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[2,"041001014010",null,"拆除原有找平层及水稳层",null,"1.名称：破碎地面\n2.满足设计及相关规范要求",null,"1000m3",0.044625]
[3,"040105008006",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.044625]
[4,"040105009008",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.044625]
[5,"040204001001",null,"人行道整形碾压",null,"1.名称：路床碾压\n2.满足图纸及规范设计要求",null,"100m2",1.275]
[6,"040204002017",null,"人行道块料铺设 水泥砂浆 规格20*10*6cm",null,"1.名称：步道砖铺设\n2.做法：预制砼彩色步砖200*100*60\n3.满足图纸及规范设计要求",null,"100m2",1.275]
[7,"040202032016",null,"厂拌水泥稳定砂砾(50m2以外) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",1.275]
[8,"040204010009",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.95917]
[9,"040204006025",null,"检查井、窨井 升高30cm",null,"1.调整检查井\n2.部位：沥青路面上的检查井调整高度同路面\n3.满足图纸及相关规范设计要求",null,"座",4]
[10,"040101003013",null,"人工挖基坑土方 一、二类土深度在2m以内",null,"1.名称：人工挖土\n2.土壤类别：一、二类土\n3.满足图纸及规范设计要求",null,"100m3",0.6375]
[11,"040104006019",null,"挖掘机装土方 挖掘机1m3",null,"1.名称：土方装车\n2.满足图纸及规范设计要求",null,"1000m3",0.06375]
[12,"040104006020",null,"自卸汽车运土方 运距≤1km",null,"1.名称：土方外运\n2.做法：运距10km\n3.满足设计及相关规范要求",null,"1000m3",0.06375]
[13,"040103003005",null,"直埋管沟回填 砂",null,"1.名称：回填砂\n2.满足设计及相关规范要求",null,"10m3",8.925]
[14,"040503002002",null,"混凝土支墩 管道支墩(挡墩) ",null,"1.名称：砼支墩\n2.做法：C15混凝土；",null,"10m3",0.15]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  11  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":3},"每处3m3内",null,"1m*1m*1.5m\n3.满足设计及相关规范要求"]
[15,"040901009001",null,"铁件制安 预埋铁件",null,"1.名称：预埋件\n2.满足设计及相关规范要求",null,"t",0.02014]
[16,"04003",null,"抢修焊管用焊工",null,"1.满足设计及相关规范要求",null,"工日",1]
[{"$nulls":3},"加工区15D厂房南侧荷兰砖地面修缮"]
[1,"041001002008",null,"拆除人行道 荷兰砖",null,"1.名称：拆除荷兰砖\n2.满足设计及相关规范要求",null,"100m2",0.275]
[2,"041001014012",null,"拆除原有水稳层",null,"1.名称：拆除原有水稳层\n2.满足设计及相关规范要求",null,"1000m3",0.00825]
[3,"040105008008",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.011]
[4,"040105009010",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.011]
[5,"040204001003",null,"人行道整形碾压",null,"1.名称：路床碾压\n2.满足图纸及规范设计要求",null,"100m2",0.275]
[6,"040204002045",null,"人行道块料铺设 水泥砂浆 规格20*10*6cm(利旧)",null,"1.名称：步道砖铺设\n2.做法：预制砼彩色步砖200*100*60(利旧)\n3.满足图纸及规范设计要求",null,"100m2",0.275]
[7,"040202032018",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.275]
[8,"040204010011",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.20688]
[{"$nulls":3},"加工区29E-1E，转盘方井修缮"]
[1,"041001002009",null,"拆除人行道 荷兰砖",null,"1.名称：拆除荷兰砖\n2.满足设计及相关规范要求",null,"100m2",1.5611]
[2,"041001014013",null,"拆除原有水稳层",null,"1.名称：拆除原有水稳层",null,"1000m3",0.046833]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  12  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":5},"2.满足设计及相关规范要求"]
[3,"040105008009",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.062444]
[4,"040105009011",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.062444]
[5,"040204001004",null,"人行道整形碾压",null,"1.名称：路床碾压\n2.满足图纸及规范设计要求",null,"100m2",1.5611]
[6,"040204002046",null,"人行道块料铺设 水泥砂浆 规格20*10*6cm(利旧、增加11.1m2新砖）",null,"1.名称：步道砖铺设\n2.做法：预制砼彩色步砖200*100*60(利旧、增加11.1m2新砖）\n3.满足图纸及规范设计要求",null,"100m2",1.5611]
[7,"040202032019",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",1.5611]
[8,"040204010012",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",1.1744]
[9,"040204006019",null,"拆安树木防护套",{"$nulls":3},"座",4]
[10,"041001005008",null,"边石拆除",null,"1.边石拆除\n2.满足图纸及规范设计要求",null,"100m",0.34]
[11,"040204004037",null,"边石安装100*100mm（利旧）",null,"1.边石安装100*100mm\n2.满足图纸及规范设计要求",null,"100m",0.34]
[12,"040204004038",null,"人工铺装垫层 预拌混凝土",null,"1.名称：混凝土地面\n2.做法：混凝土垫层\n3.满足图纸及相关规范设计要求",null,"10m3",0.068]
[13,"040504001049",null,"砖砌方井1.1*1.1*1",null,"1.名称：砌筑方井\n2.满足设计及相关规范要求",null,"座",1]
[{"$nulls":3},"加工区29E更换玻璃"]
[{"$nulls":3},"加工区VAC车棚修缮"]
[{"$nulls":3},"加工区平水泵房散水及道路"]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  13  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[1,"041001014015",null,"拆除原有砼路面",null,"1.名称：拆除原有砼路面\n2.满足设计及相关规范要求",null,"1000m3",0.003366]
[2,"040105008011",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.003366]
[3,"040105009013",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.003366]
[4,"040104003046",null,"反铲挖掘机挖槽坑土方 一、二类土",null,"1.名称：机械挖土\n2.土壤类别：一、二类土\n3.满足图纸及规范设计要求",null,"1000m3",0.005049]
[5,"040104006025",null,"挖掘机装土方 挖掘机1m3",null,"1.名称：土方装车\n2.满足图纸及规范设计要求",null,"1000m3",0.005049]
[6,"040104006026",null,"自卸汽车运土方 运距≤1km",null,"1.名称：土方外运\n2.做法：运距10km\n3.满足设计及相关规范要求",null,"1000m3",0.005049]
[7,"040204004039",null,"混凝土200mm厚c30细石混凝土",null,"1.名称：混凝土地面\n2.做法：C30细石混凝土 200mm厚\n3.满足图纸及相关规范设计要求",null,"10m3",0.3366]
[8,"040901001001",null,"现浇构件圆钢筋 钢丝 直径4mm",null,"1.规格：一级钢筋4\n2.钢筋制作、运输、绑扎、安装\n3.满足图纸及相关规范设计要求",null,"t",0.019547]
[9,"040202032020",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.1683]
[10,"040204010014",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.12661]
[11,"041001005002",null,"边石拆除",null,"1.边石拆除\n2.满足图纸及规范设计要求",null,"100m",0.148]
[12,"040204004013",null,"边石安装100*100mm（利旧）",null,"1.边石安装100*100mm\n2.满足图纸及规范设计要求",null,"100m",0.148]
[13,"040204004040",null,"人工铺装垫层 预拌混凝土",null,"1.名称：混凝土地面\n2.做法：混凝土垫层",null,"10m3",0.0296]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  14  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[{"$nulls":5},"3.满足图纸及相关规范设计要求"]
[{"$nulls":3},"加工区转盘地面"]
[1,"041001002008",null,"拆除人行道 块料面层",null,"1.名称：步道砖拆除\n2.满足规范及设计要求",null,"100m2",0.10799]
[2,"011616001015",null,"建筑垃圾外运 运距10000m",null,"1.名称：建筑垃圾外运\n2.做法：运距10km\n3.满足规范及设计要求",null,"10m3",0.043196]
[3,"011102001007",null,"原有地面重新铺火烧板（利旧）",null,"1.名称：重铺火烧板\n2.做法：主材利旧\n3.满足规范及设计要求",null,"100m2",0.0432]
[4,"040204002032",null,"原有地面重新铺火烧板",{"$nulls":3},"100m2",0.10799]
[{"$nulls":3},"加工区42G北侧下水管维修"]
[1,"040203014006",null,"切割机切割路面 沥青混凝土路面 厚度10cm以内",null,"1.切割路面\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m",0.07]
[2,"041001001010",null,"拆除沥青柏油类路面层 小型机械拆除 厚10cm厚",null,"1.沥青路面拆除\n2.满足图纸及规范设计要求",null,"100m2",0.03]
[3,"041001014012",null,"液压岩石破碎机破碎砼及钢筋砼 沥青混凝土面层、半刚性材料",null,"1.路基拆除\n2.满足图纸及规范设计要求",null,"1000m3",0.0009]
[4,"040105008012",null,"机械装石渣",null,"1.机械装石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.0012]
[5,"040105009014",null,"运石渣 运距10km",null,"1.机械运石渣\n2.满足图纸及规范设计要求",null,"1000m3",0.0012]
[6,"040101003001",null,"人工挖基坑土方 一、二类土深度在2m以内",null,"1.名称：挖土方\n2.满足设计及相关规范要求",null,"100m3",0.033]
[7,"010101007010",null,"人工装车 土方",null,"1.名称：装土方\n2.满足设计及相关规范要求",null,"10m3",0.33]
[8,"040104006011",null,"小型自卸汽车运土方 运距≤1km",null,"1.名称：运土方\n2.满足设计及相关规范要求",null,"1000m3",0.0033]
[9,"040103003006",null,"直埋管沟回填 砂",null,"1.名称：回填砂\n2.满足设计及相关规范要求",null,"10m3",0.33]
["本页小计"]
[{"$nulls":11},"表—08"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：加工区市政零散维修-01",{"$nulls":5},"标段：",{"$nulls":4},"第  15  页  共  15  页"]
["序号","项目编码",null,"项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":10},"综合单价",null,"合价","其中"]
[{"$nulls":13},"人工费+机械费"]
[10,"040202001007",null,"路床整形 路床碾压检验",null,"1.路床碾压\n2.满足图纸及规范设计要求",null,"100m2",0.03]
[11,"040202032021",null,"厂拌水泥稳定砂砾(50m2以内) 水泥含量6% 厚度30cm",null,"1.30cm厚水泥稳定砂砾（水泥含量6%）\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.03]
[12,"040202036010",null,"基层养生 塑料膜养生",null,"1.基层养生\n2.满足图纸及规范设计要求",null,"100m2",0.03]
[13,"040203003019",null,"透层 半刚性基层 乳化沥青 0.7kg/m2",null,"1.透层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.003]
[14,"040203003020",null,"黏(粘)层 沥青层 乳化沥青 0.3kg/m2",null,"1.黏层\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"1000m2",0.003]
[15,"040203006043",null,"沥青混凝土路面 中粒式 机械摊铺50m2以内 厚度6cm",null,"1.6cm厚中粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.03]
[16,"040203006044",null,"沥青混凝土路面 细粒式 机械摊铺50m2以内 厚度4cm",null,"1.4cm厚细粒式沥青混凝土\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100m2",0.03]
[17,"040204010015",null,"水泥稳定粒料 自卸汽车运输 运距15km以内",null,"1.水稳运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.022569]
[18,"040204011010",null,"沥青混凝土 自卸汽车运输 运距15km以内",null,"1.沥青混凝土运输\n2.部位：沥青路面\n3.满足图纸及相关规范设计要求",null,"100t",0.007351]
[]
[]
[]
[]
[]
[]
["本页小计"]
["合    计"]
[{"$nulls":11},"表—08"]