{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["表2"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"表2","index":0,"n_rows":30,"n_cols":12,"rows_kept":30,"merged":[[0,0,0,8],[0,9,0,11],[1,0,3,0],[1,1,3,2],[1,3,3,4],[1,5,3,5],[1,6,3,7],[1,8,1,11],[2,8,3,9],[2,10,3,10],[2,11,3,11],[4,1,4,2],[4,3,4,4],[4,6,4,7],[4,8,4,9],[5,1,5,2],[5,3,5,4],[5,6,5,7],[5,8,5,9],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[9,1,9,2],[9,3,9,4],[9,6,9,7],[9,8,9,9],[10,1,10,2],[10,3,10,4],[10,6,10,7],[10,8,10,9],[11,1,11,2],[11,3,11,4],[11,6,11,7],[11,8,11,9],[12,1,12,2],[12,3,12,4],[12,6,12,7],[12,8,12,9],[13,1,13,2],[13,3,13,4],[13,6,13,7],[13,8,13,9],[14,1,14,2],[14,3,14,4],[14,6,14,7],[14,8,14,9],[15,1,15,2],[15,3,15,4],[15,6,15,7],[15,8,15,9],[16,1,16,2],[16,3,16,4],[16,6,16,7],[16,8,16,9],[17,1,17,2],[17,3,17,4],[17,6,17,7],[17,8,17,9],[18,1,18,2],[18,3,18,4],[18,6,18,7],[18,8,18,9],[19,1,19,2],[19,3,19,4],[19,6,19,7],[19,8,19,9],[20,1,20,2],[20,3,20,4],[20,6,20,7],[20,8,20,9],[21,1,21,2],[21,3,21,4],[21,6,21,7],[21,8,21,9],[22,1,22,2],[22,3,22,4],[22,6,22,7],[22,8,22,9],[23,1,23,2],[23,3,23,4],[23,6,23,7],[23,8,23,9],[24,1,24,2],[24,3,24,4],[24,6,24,7],[24,8,24,9],[25,1,25,2],[25,3,25,4],[25,6,25,7],[25,8,25,9],[26,1,26,2],[26,3,26,4],[26,6,26,7],[26,8,26,9],[27,1,27,2],[27,3,27,4],[27,6,27,7],[27,8,27,9],[28,0,28,9],[29,0,29,9],[30,2,30,3],[30,4,30,6],[30,7,30,8],[30,9,30,11]],"flags":["formulas_cached_only"]}
["附件二"]
["序号","项目名称",null,"项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","备注"]
[]
[null,"给水系统"]
[1,"室内塑料给水管(热熔连接) 外径25mm以内",null,"1.名称：给水管\n2.规格：DN20\n3.材质：PP-R塑料管 S5级\n4.连接方式：热熔连接\n5.包含管道及管件安装、水压试验及水冲洗\n6.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",0.367]
[2,"室内塑料给水管(热熔连接) 外径20mm以内",null,"1.名称：给水管\n2.规格：DN15\n3.材质：PP-R塑料管 S5级\n4.连接方式：热熔连接\n5.包含管道及管件安装、水压试验及水冲洗\n6.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",0.819]
[3,"管道消毒、冲洗 公称直径50mm以内",null,"1.名称：管道消毒、冲洗 公称直径50mm以内\n2.备注：满足招标文件、图纸设计及施工规范要求",null,"100m",0.1186]
[4,"普通水表安装(螺纹连接) 公称直径20mm以内",null,"1.名称：水表\n2.规格型号：DN20\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",1]
[5,"螺纹阀门安装 公称直径20mm以内",null,"1.名称：铜制截止阀\n2.规格：DN20\n3.材质：全铜\n4.连接方式：螺纹连接\n5.备注：满足招标文件、图纸设计及施工规范要求",null,"个",1]
[6,"螺纹阀门安装 公称直径15mm以内",null,"1.名称：铜制截止阀\n2.规格：DN15\n3.材质：全铜\n4.连接方式：螺纹连接\n5.备注：满足招标文件、图纸设计及施工规范要求",null,"个",1]
[7,"成品管卡安装 公称直径20mm以内",null,"1.名称：成品管卡安装\n2.规格型号：DN20\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",3]
[8,"成品管卡安装 公称直径20mm以内",null,"1.名称：成品管卡安装\n2.规格型号：DN15\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",3]
[9,"机械钻孔 混凝",null,"1.名称：水钻打孔 钻孔",null,"10个",0.1]
[null,"土墙体钻孔 钻孔直径83mm以内",null,"直径83mm以内\n2.备注：满足招标文件、图纸设计及施工规范要求"]
[null,"排水系统"]
[1,"室内塑料排水管(粘接) 外径110mm以内",null,"1.名称：排水管\n2.规格：DN100\n3.材质：U-PVC 塑料管\n4.连接方式：粘接\n5.包含管道及管件安装、灌水试验\n6.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",0.445]
[2,"室内塑料排水管(粘接) 外径50mm以内",null,"1.名称：排水管\n2.规格：DN50\n3.材质：U-PVC 塑料管\n4.连接方式：粘接\n5.包含管道及管件安装、灌水试验\n6.备注：满足招标文件、图纸设计及施工规范要求",null,"10m",0.86]
[3,"台下盆",null,"1.名称：台下盆（304不锈钢）\n2.包含304净水龙头、304洗杯器、503过滤网、托架及卫生洁具附件\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"10组",0.1]
[4,"成品管卡安装 公称直径100mm以内",null,"1.名称：成品管卡安装\n2.规格型号：DN100\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",3]
[5,"成品管卡安装 公称直径50mm以内",null,"1.名称：成品管卡安装\n2.规格型号：DN50\n3.备注：满足招标文件、图纸设计及施工规范要求",null,"个",2]
[null,"安装费用"]
[1,"给排水、采暖、燃气工程 脚手架搭拆费",{"$nulls":3},"项",1]
[]
[]
[]
[]
[]
["本页小计"]
["合   计"]